Labels And Decals

Labels
Materials needed:

Image
Photo Editor (Photo Shop, GIMP)
Printer
Labels (Avery Shipping Labels)
Tube
Clear Acrylic Spray

· Once an image is selected use a photo editor to crop it as desired and add a thin border to it.  It may then be sized to the circumference and length of your tube.

· To determine circumference you need to know that Pi = 3.14

· Using a Sierra tube as an example:

A Sierra tube is 2.21” long
The diameter of a Sierra tube is .41

Pi x D =C

3.14 x .41 = 1.2874

Add ..0625” (1/16”) to each measurement to allow a slight overlap, overhang.

Tube length 2.21 + .0625 = 2.2725
Tube Circumference 1.2874 + .0625 = 1.3499

The image that you apply to the tube needs to be 2.27 x 1.35.  

· Print your correctly sized image and let it dry for 24 hours.

· Cut your printed image out of the Avery label.

· When you apply the label to your tube it should overlap  You will want to hide the white edge of the label that will be exposed .  Before you apply the label use a Sharpie Permanent Marker that is close to the color of your border. and color the edge of the label that will overlap the other side.

· Once the .Label is applied seal it with the Clear Acrylic Spray and let it dry for 24 hours.

· Cast using your preferred method.

Decals

Materials Needed:

Image
Photo Editor (Photo Shop, GIMP)
Printer
Decal Paper (www.decalpaper.com be sure to get clear)
Blank turned slightly under size
Micro-Sol
Clear Acrylic Spray

· Select image and/or text and print on decal paper
Allow to dry for 24 hours

· Seal with clear acrylic spray
Allow to dry for 24 hours

· Cut decal from paper and apply to blank

· Top with Micro-Sol
Allow to dry for 24 hours

· Apply CA until edges are smooth


